#Error messages
none = OK.
0 = Unspecified error.
1 = High temperature.
2 = Shutdown temperature.
3 = High reflection.
4 = Shutdown reflection.
5 = Reset detected.
6 = Temperature measurement failure.
7 = Power measurement failure.
8 = RF enable failure.
9 = Multiplexer failure.
10 = External shutdown detected.
11 = Out of memory.
12 = I2C error.
13 = SPI error.
14 = IQ conversion error.
15 = SOA measurement error.
16 = External watchdog timeout.
17 = Calibration missing.
18 = External protection triggered.
19 = SOA high dissipation.
20 = SOA shutdown dissipation.
21 = Calibration EEPROM outdated.
22 = PA error.
23 = PA reset failure.
24 = PA high current.
25 = IQ demodulator lock lost.
26 = Alarm IN signaled.
27 = IQ modulator lock lost.
28 = SOA high current.
29 = SOA shutdown current.
30 = SOA high forward power.
31 = SOA shutdown forward power.
32 = SOA shutdown minimum voltage.
33 = SOA low voltage.
34 = SOA high voltage.
35 = SOA shutdown maximum voltage.
else = Unknown error. 
